**“Debody" technical rider.**

**GENERAL:**

This technical outline is an integral part of the contract between the producer and the organizer of the performance. This means that the organizer should fulfill the technical conditions on his initiative and expenses. Exceptions are only possible if confirmed in writing.

Therefore the organizer should provide a technical rider of the space to the

company (dimensions, list of normally available equipment, floor plan, cross - section on scale). On the basis of this we can look for adaptations.

**STAGE REQUIREMENTS:**

Space approx. 9x10 meters

Black dance floor

Truss system approx. 5.5 meters high

**LIGHTNING REQUIREMENTS:**

24 circuits

2 kW per circuit

Programmable lightning console with min 24 submasters

PC 1000W –16 pcs

Fresnel 1000W – 3 pcs

Profile 575W –2pcs

Flood 1000W – 2 pcs

Pin Spot -. 13 pcs

Light for the audience dimmable from lightning console

**VIDEO REQUIREMENTS**

Back wall should be suitable for the video projection(white screen or white-drop preferred). Possibility to hang a beamer. Beamer is provided by company. Video technician is situated near the light technician in the booth.

**STAFF REQUIREMENTS:**

Light technician - 1

Stage technician - 1

**OTHER REQUIREMENTS:**

Dressing room for 4 persons

Bottled water

Set up approx. 8 hours

Strike approx. 2 hours

Duration of the show approx. 30 minutes

In any question please contact us personally.

Ints Plavnieks

Tel: +421944167466

[inc@stanica.sk](mailto:inc@stanica.sk)

---www.stanica.sk---